From 33239152305567b3e9bf052f71fd4baecd626341 Mon Sep 17 00:00:00 2001
From: Sergio Paracuellos <sergio.paracuellos@gmail.com>
Date: Tue, 10 Sep 2024 06:40:22 +0200
Subject: [PATCH 1/3] clk: ralink: mtmips: fix clock plan for Ralink SoC RT3883

Clock plan for Ralink SoC RT3883 needs an extra 'periph' clock to properly
set some peripherals that has this clock as their parent. When this driver
was mainlined we could not find any active users of this SoC so we cannot
perform any real tests for it. Now, one user of a Belkin f9k1109 version 1
device which uses this SoC appear and reported some issues in openWRT:
- https://github.com/openwrt/openwrt/issues/16054
The peripherals that are wrong are 'uart', 'i2c', 'i2s' and 'uartlite' which
has a not defined 'periph' clock as parent. Hence, introduce it to have a
properly working clock plan for this SoC.

Fixes: 6f3b15586eef ("clk: ralink: add clock and reset driver for MTMIPS SoCs")
Signed-off-by: Sergio Paracuellos <sergio.paracuellos@gmail.com>
Link: https://lore.kernel.org/r/20240910044024.120009-2-sergio.paracuellos@gmail.com
Signed-off-by: Stephen Boyd <sboyd@kernel.org>
---
 drivers/clk/ralink/clk-mtmips.c | 9 +++++++--
 1 file changed, 7 insertions(+), 2 deletions(-)

--- a/drivers/clk/ralink/clk-mtmips.c
+++ b/drivers/clk/ralink/clk-mtmips.c
@@ -267,6 +267,11 @@ static struct mtmips_clk_fixed rt305x_fi
 	CLK_FIXED("xtal", NULL, 40000000)
 };
 
+static struct mtmips_clk_fixed rt3883_fixed_clocks[] = {
+	CLK_FIXED("xtal", NULL, 40000000),
+	CLK_FIXED("periph", "xtal", 40000000)
+};
+
 static struct mtmips_clk_fixed rt3352_fixed_clocks[] = {
 	CLK_FIXED("periph", "xtal", 40000000)
 };
@@ -779,8 +784,8 @@ static const struct mtmips_clk_data rt33
 static const struct mtmips_clk_data rt3883_clk_data = {
 	.clk_base = rt3883_clks_base,
 	.num_clk_base = ARRAY_SIZE(rt3883_clks_base),
-	.clk_fixed = rt305x_fixed_clocks,
-	.num_clk_fixed = ARRAY_SIZE(rt305x_fixed_clocks),
+	.clk_fixed = rt3883_fixed_clocks,
+	.num_clk_fixed = ARRAY_SIZE(rt3883_fixed_clocks),
 	.clk_factor = NULL,
 	.num_clk_factor = 0,
 	.clk_periph = rt5350_pherip_clks,
