// SPDX-License-Identifier: GPL-2.0-or-later

#include "bcm6328.dtsi"

/ {
	model = "Sercomm AD1018";
	compatible = "sercomm,ad1018", "brcm,bcm6328";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_power_green;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		wps {
			label = "wps";
			gpios = <&gpio 24 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};

		wlan {
			label = "wlan";
			gpios = <&gpio 25 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WLAN>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&gpio 31 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};
	};

	bcm432217-sprom {
		compatible = "brcm,bcma-sprom";

		pci-bus = <1>;
		pci-dev = <0>;

		nvmem-cells = <&macaddr_cferom_6a0 1>;
		nvmem-cell-names = "mac-address";

		brcm,sprom = "brcm/bcm43217-sprom.bin";
		brcm,sprom-fixups = <6 0x1c00>,
				    <65 0x1256>,
				    <96 0x2046>,
				    <97 0xfe69>,
				    <98 0x1726>,
				    <99 0xfa5c>,
				    <112 0x2046>,
				    <113 0xfea8>,
				    <114 0x1978>,
				    <115 0xfa26>,
				    <161 0x2222>,
				    <169 0x2222>,
				    <171 0x2222>,
				    <173 0x2222>,
				    <174 0x4444>,
				    <175 0x2222>,
				    <176 0x4444>;
	};
};

&ehci {
	status = "okay";
};

&ethernet {
	status = "okay";

	nvmem-cells = <&macaddr_cferom_6a0 0>;
	nvmem-cell-names = "mac-address";
};

&leds {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_leds &pinctrl_serial_led
		     &pinctrl_ephy0_spd_led &pinctrl_ephy1_act_led
		     &pinctrl_ephy2_act_led &pinctrl_ephy3_act_led>;

	brcm,serial-leds;
	brcm,serial-shift-inv;
	brcm,serial-dat-low;

	led@0 {
		reg = <0>;
		active-low;
		label = "red:internet";
	};

	led@1 {
		reg = <1>;
		active-low;
		label = "green:internet";
	};

	led_power_green: led@8 {
		reg = <8>;
		active-low;
		function = LED_FUNCTION_POWER;
		color = <LED_COLOR_ID_GREEN>;
	};

	led@10 {
		reg = <10>;
		active-low;
		label = "green:adsl";
	};

	led@11 {
		reg = <11>;
		active-low;
		label = "red:adsl";
	};

	led@12 {
		reg = <12>;
		active-low;
		label = "green:phone";
	};

	led@13 {
		reg = <13>;
		active-low;
		function = LED_FUNCTION_WPS;
		color = <LED_COLOR_ID_GREEN>;
	};

	led@14 {
		reg = <14>;
		active-low;
		label = "green:wifi";
	};

	led@15 {
		reg = <15>;
		active-low;
		function = LED_FUNCTION_USB;
		color = <LED_COLOR_ID_GREEN>;
	};

	led@17 {
		/* EPHY0 Spd */
		reg = <17>;
		brcm,hardware-controlled;
	};
};

&ohci {
	status = "okay";
};

&pcie {
	status = "okay";
};

&pinctrl {
	pinctrl_leds: leds {
		function = "led";
		pins = "gpio0", "gpio1";
	};
};

&nflash {
	status = "okay";

	nandcs@0 {
		compatible = "brcm,nandcs";
		reg = <0>;
		nand-ecc-step-size = <512>;
		nand-ecc-strength = <15>;
		nand-on-flash-bbt;

		#address-cells = <1>;
		#size-cells = <1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "cferom";
				reg = <0x0000000 0x0020000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_cferom_6a0: macaddr@6a0 {
						compatible = "mac-base";
						reg = <0x6a0 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			partition@20000 {
				label = "mmap";
				reg = <0x0020000 0x00a0000>;
				read-only;
			};

			partition@c0000 {
				label = "cferam1";
				reg = <0x00c0000 0x0140000>;
				read-only;
			};

			partition@200000 {
				label = "cferam2";
				reg = <0x0200000 0x0140000>;
				read-only;
			};

			partition@340000 {
				label = "serial";
				reg = <0x0340000 0x00a0000>;
				read-only;
			};

			partition@3e0000 {
				label = "protect";
				reg = <0x03e0000 0x0140000>;
				read-only;
			};

			partition@6920000 {
				label = "bootflag1";
				reg = <0x6920000 0x0140000>;
				read-only;
			};

			partition@6a60000 {
				label = "bootflag2";
				reg = <0x6a60000 0x0140000>;
				read-only;
			};

			partition@520000 {
				compatible = "sercomm,wfi";
				label = "wfi";
				reg = <0x0520000 0x6400000>;
			};

			partition@6ba0000 {
				label = "xml_cfg";
				reg = <0x6ba0000 0x0280000>;
				read-only;
			};

			partition@6e20000 {
				label = "app_dat";
				reg = <0x6e20000 0x0280000>;
				read-only;
			};
		};
	};
};

&switch0 {
	ports {
		port@0 {
			reg = <0>;
			label = "fibre";

			phy-handle = <&phy1>;
			phy-mode = "mii";
		};

		port@1 {
			reg = <1>;
			label = "lan3";

			phy-handle = <&phy2>;
			phy-mode = "mii";
		};

		port@2 {
			reg = <2>;
			label = "lan2";

			phy-handle = <&phy3>;
			phy-mode = "mii";
		};

		port@3 {
			reg = <3>;
			label = "lan1";

			phy-handle = <&phy4>;
			phy-mode = "mii";
		};
	};
};

&uart0 {
	status = "okay";
};

&usbh {
	status = "okay";
};
