# SPDX-License-Identifier: GPL-2.0-or-later

. /lib/functions/leds.sh
. /lib/functions/uci-defaults.sh

board_config_update

case "$(board_name)" in
huawei,hg253s-v2)
	ucidef_set_led_usbport "usb" "USB" "green:usb" "usb1-port1" "usb2-port1"
	;;
netgear,dgnd3700-v2)
	ucidef_set_led_usbport "usb1" "USB1" "green:usb1" "usb1-port1" "usb2-port1"
	ucidef_set_led_usbport "usb2" "USB2" "green:usb2" "usb1-port2" "usb2-port2"
	;;
esac

board_config_flush

exit 0
