From fa7de9a76b91e1a2c4fe623e5b6fbbb704b76c5f Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Tue, 10 Nov 2020 11:21:56 +0000
Subject: [PATCH 0264/1085] drm/panel/raspberrypi-ts: Insert delay before
 polling for startup state

In switching to the hardware I2C controller there is an issue
where we seem to not get back the correct state from the Pi
touchscreen.
Insert a delay before polling to avoid this condition.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/gpu/drm/panel/panel-raspberrypi-touchscreen.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/gpu/drm/panel/panel-raspberrypi-touchscreen.c
+++ b/drivers/gpu/drm/panel/panel-raspberrypi-touchscreen.c
@@ -298,6 +298,7 @@ static int rpi_touchscreen_prepare(struc
 	int i;
 
 	rpi_touchscreen_i2c_write(ts, REG_POWERON, 1);
+	usleep_range(20000, 25000);
 	/* Wait for nPWRDWN to go low to indicate poweron is done. */
 	for (i = 0; i < 100; i++) {
 		if (rpi_touchscreen_i2c_read(ts, REG_PORTB) & 1)
