From 9e1faff1cbc877903d019a7943d37ddc5042704d Mon Sep 17 00:00:00 2001
From: John Clark <inindev@gmail.com>
Date: Thu, 28 Dec 2023 17:29:35 +0000
Subject: [PATCH] arm64: dts: rockchip: nanopc-t6 sdmmc beautification

drop max-frequency = <200000000> as it is already defined in rk3588s.dtsi
order no-sdio & no-mmc properties while we are here

Signed-off-by: John Clark <inindev@gmail.com>
Link: https://lore.kernel.org/r/20231228173011.2863-1-inindev@gmail.com
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dts | 5 ++---
 1 file changed, 2 insertions(+), 3 deletions(-)

--- a/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588-nanopc-t6.dts
@@ -536,13 +536,12 @@
 };
 
 &sdmmc {
-	max-frequency = <200000000>;
-	no-sdio;
-	no-mmc;
 	bus-width = <4>;
 	cap-mmc-highspeed;
 	cap-sd-highspeed;
 	disable-wp;
+	no-mmc;
+	no-sdio;
 	sd-uhs-sdr104;
 	vmmc-supply = <&vcc_3v3_s3>;
 	vqmmc-supply = <&vccio_sd_s0>;
