From 158032d3d4e5089afa2aa38c27c6e222ac427820 Mon Sep 17 00:00:00 2001
From: Robert Marko <robimarko@gmail.com>
Date: Thu, 20 May 2021 14:57:46 +0200
Subject: [PATCH 4/8] EDMA: Use NAPI_POLL_WEIGHT as NAPI weight

Currently a weight of 100 is used by the EDMA, according
to upstream max of 64 should be used and that is used for
almost any driver.

They also introduced NAPI_POLL_WEIGHT define which equals
to 64.

So use NAPI_POLL_WEIGHT as the weight.

Signed-off-by: Robert Marko <robimarko@gmail.com>
---
 hal/dp_ops/edma_dp/edma_v1/edma_data_plane.c | 2 +-
 hal/dp_ops/edma_dp/edma_v1/edma_data_plane.h | 1 -
 2 files changed, 1 insertion(+), 2 deletions(-)

--- a/hal/dp_ops/edma_dp/edma_v1/edma_data_plane.c
+++ b/hal/dp_ops/edma_dp/edma_v1/edma_data_plane.c
@@ -845,7 +845,7 @@ static int edma_register_netdevice(struc
 	 */
 	if (!edma_hw.napi_added) {
 		netif_napi_add(netdev, &edma_hw.napi, edma_napi,
-				EDMA_NAPI_WORK);
+				NAPI_POLL_WEIGHT);
 		/*
 		 * Register the interrupt handlers and enable interrupts
 		 */
--- a/hal/dp_ops/edma_dp/edma_v1/edma_data_plane.h
+++ b/hal/dp_ops/edma_dp/edma_v1/edma_data_plane.h
@@ -26,7 +26,6 @@
 #define EDMA_RX_PREHDR_SIZE		(sizeof(struct edma_rx_preheader))
 #define EDMA_TX_PREHDR_SIZE		(sizeof(struct edma_tx_preheader))
 #define EDMA_RING_SIZE			128
-#define EDMA_NAPI_WORK			100
 #define EDMA_START_GMACS		NSS_DP_HAL_START_IFNUM
 #define EDMA_MAX_GMACS			NSS_DP_HAL_MAX_PORTS
 #define EDMA_TX_PKT_MIN_SIZE		33	/* IPQ807x EDMA needs a minimum packet size of 33 bytes */
