From: Aditya Kumar Singh <quic_adisi@quicinc.com>
Date: Fri, 6 Sep 2024 12:14:19 +0530
Subject: [PATCH] Revert "wifi: mac80211: move radar detect work to sdata"
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This reverts commit ce9e660ef32e ("wifi: mac80211: move radar detect work to sdata").

To enable radar detection with MLO, it’s essential to handle it on a
per-link basis. This is because when using MLO, multiple links may already
be active and beaconing. In this scenario, another link should be able to
initiate a radar detection. Also, if underlying links are associated with
different hardware devices but grouped together for MLO, they could
potentially start radar detection simultaneously. Therefore, it makes
sense to manage radar detection settings separately for each link by moving
them back to a per-link data structure.

Signed-off-by: Aditya Kumar Singh <quic_adisi@quicinc.com>
Link: https://patch.msgid.link/20240906064426.2101315-2-quic_adisi@quicinc.com
Signed-off-by: Johannes Berg <johannes.berg@intel.com>
---

--- a/net/mac80211/cfg.c
+++ b/net/mac80211/cfg.c
@@ -1658,7 +1658,7 @@ static int ieee80211_stop_ap(struct wiph
 
 	if (sdata->wdev.cac_started) {
 		chandef = link_conf->chanreq.oper;
-		wiphy_delayed_work_cancel(wiphy, &sdata->dfs_cac_timer_work);
+		wiphy_delayed_work_cancel(wiphy, &link->dfs_cac_timer_work);
 		cfg80211_cac_event(sdata->dev, &chandef,
 				   NL80211_RADAR_CAC_ABORTED,
 				   GFP_KERNEL);
@@ -3482,7 +3482,7 @@ static int ieee80211_start_radar_detecti
 	if (err)
 		goto out_unlock;
 
-	wiphy_delayed_work_queue(wiphy, &sdata->dfs_cac_timer_work,
+	wiphy_delayed_work_queue(wiphy, &sdata->deflink.dfs_cac_timer_work,
 				 msecs_to_jiffies(cac_time_ms));
 
  out_unlock:
@@ -3499,7 +3499,7 @@ static void ieee80211_end_cac(struct wip
 
 	list_for_each_entry(sdata, &local->interfaces, list) {
 		wiphy_delayed_work_cancel(wiphy,
-					  &sdata->dfs_cac_timer_work);
+					  &sdata->deflink.dfs_cac_timer_work);
 
 		if (sdata->wdev.cac_started) {
 			ieee80211_link_release_channel(&sdata->deflink);
--- a/net/mac80211/ieee80211_i.h
+++ b/net/mac80211/ieee80211_i.h
@@ -1069,6 +1069,7 @@ struct ieee80211_link_data {
 	int ap_power_level; /* in dBm */
 
 	bool radar_required;
+	struct wiphy_delayed_work dfs_cac_timer_work;
 
 	union {
 		struct ieee80211_link_data_managed mgd;
@@ -1167,8 +1168,6 @@ struct ieee80211_sub_if_data {
 	struct ieee80211_link_data deflink;
 	struct ieee80211_link_data __rcu *link[IEEE80211_MLD_MAX_NUM_LINKS];
 
-	struct wiphy_delayed_work dfs_cac_timer_work;
-
 	/* for ieee80211_set_active_links_async() */
 	struct wiphy_work activate_links_work;
 	u16 desired_active_links;
--- a/net/mac80211/iface.c
+++ b/net/mac80211/iface.c
@@ -551,7 +551,7 @@ static void ieee80211_do_stop(struct iee
 	wiphy_work_cancel(local->hw.wiphy,
 			  &sdata->deflink.color_change_finalize_work);
 	wiphy_delayed_work_cancel(local->hw.wiphy,
-				  &sdata->dfs_cac_timer_work);
+				  &sdata->deflink.dfs_cac_timer_work);
 
 	if (sdata->wdev.cac_started) {
 		chandef = sdata->vif.bss_conf.chanreq.oper;
@@ -1744,8 +1744,6 @@ static void ieee80211_setup_sdata(struct
 	wiphy_work_init(&sdata->work, ieee80211_iface_work);
 	wiphy_work_init(&sdata->activate_links_work,
 			ieee80211_activate_links_work);
-	wiphy_delayed_work_init(&sdata->dfs_cac_timer_work,
-				ieee80211_dfs_cac_timer_work);
 
 	switch (type) {
 	case NL80211_IFTYPE_P2P_GO:
--- a/net/mac80211/link.c
+++ b/net/mac80211/link.c
@@ -45,6 +45,8 @@ void ieee80211_link_init(struct ieee8021
 			  ieee80211_color_collision_detection_work);
 	INIT_LIST_HEAD(&link->assigned_chanctx_list);
 	INIT_LIST_HEAD(&link->reserved_chanctx_list);
+	wiphy_delayed_work_init(&link->dfs_cac_timer_work,
+				ieee80211_dfs_cac_timer_work);
 
 	if (!deflink) {
 		switch (sdata->vif.type) {
--- a/net/mac80211/mlme.c
+++ b/net/mac80211/mlme.c
@@ -3031,15 +3031,16 @@ void ieee80211_dynamic_ps_timer(struct t
 
 void ieee80211_dfs_cac_timer_work(struct wiphy *wiphy, struct wiphy_work *work)
 {
-	struct ieee80211_sub_if_data *sdata =
-		container_of(work, struct ieee80211_sub_if_data,
+	struct ieee80211_link_data *link =
+		container_of(work, struct ieee80211_link_data,
 			     dfs_cac_timer_work.work);
-	struct cfg80211_chan_def chandef = sdata->vif.bss_conf.chanreq.oper;
+	struct cfg80211_chan_def chandef = link->conf->chanreq.oper;
+	struct ieee80211_sub_if_data *sdata = link->sdata;
 
 	lockdep_assert_wiphy(sdata->local->hw.wiphy);
 
 	if (sdata->wdev.cac_started) {
-		ieee80211_link_release_channel(&sdata->deflink);
+		ieee80211_link_release_channel(link);
 		cfg80211_cac_event(sdata->dev, &chandef,
 				   NL80211_RADAR_CAC_FINISHED,
 				   GFP_KERNEL);
--- a/net/mac80211/util.c
+++ b/net/mac80211/util.c
@@ -3460,7 +3460,7 @@ void ieee80211_dfs_cac_cancel(struct iee
 
 	list_for_each_entry(sdata, &local->interfaces, list) {
 		wiphy_delayed_work_cancel(local->hw.wiphy,
-					  &sdata->dfs_cac_timer_work);
+					  &sdata->deflink.dfs_cac_timer_work);
 
 		if (sdata->wdev.cac_started) {
 			chandef = sdata->vif.bss_conf.chanreq.oper;
