// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7241.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/mtd/partitions/uimage.h>

/ {
	compatible = "netgear,wnr2000-v3", "qca,ar7241";
	model = "Netgear WNR2000 v3";

	chosen {
		bootargs = "console=ttyS0,115200n8";
	};

	aliases {
		led-boot = &led_power_amber;
		led-failsafe = &led_power_amber;
		led-running = &led_power_green;
		led-upgrade = &led_power_amber;
		label-mac-device = &eth1;
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&ath9k 8 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		rfkill {
			label = "rfkill";
			linux,code = <KEY_RFKILL>;
			gpios = <&ath9k 9 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		pinctrl-names = "default";
		pinctrl-0 = <&jtag_disable_pins &switch_led_disable_pins &clks_disable_pins>;

		wan_green {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};

		wan_amber {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};

		lan1_green {
			label = "green:lan1";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		lan1_amber {
			label = "amber:lan1";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		lan2_green {
			label = "green:lan2";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		lan2_amber {
			label = "amber:lan2";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};

		lan3_green {
			label = "green:lan3";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		lan3_amber {
			label = "amber:lan3";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		lan4_green {
			label = "green:lan4";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		lan4_amber {
			label = "amber:lan4";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		wps_green {
			function = LED_FUNCTION_WPS;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		led_power_green: power_green {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&ath9k 3 GPIO_ACTIVE_LOW>;
		};

		led_power_amber: power_amber {
			function = LED_FUNCTION_POWER;
			color = <LED_COLOR_ID_AMBER>;
			gpios = <&ath9k 2 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};

		wlan_blue {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&ath9k 1 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x40000 0x10000>;
			};

			partition@50000 {
				label = "firmware";
				reg = <0x50000 0x3a0000>;
				compatible = "openwrt,uimage", "denx,uimage";
				openwrt,ih-magic = <0x32303033>;
				openwrt,ih-type = <IH_TYPE_FILESYSTEM>;
			};

			partition@3f0000 {
				label = "art";
				reg = <0x3f0000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_art_0: macaddr@0 {
						compatible = "mac-base";
						reg = <0x0 0x6>;
						#nvmem-cell-cells = <1>;
					};

					macaddr_art_6: macaddr@6 {
						reg = <0x6 0x6>;
					};
				};
			};
		};
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_art_0 0>;
	nvmem-cell-names = "mac-address";
};

&eth1 {
	compatible = "qca,ar7241-eth", "syscon", "simple-mfd";

	nvmem-cells = <&macaddr_art_6>;
	nvmem-cell-names = "mac-address";
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0 {
		compatible = "pci168c,002e";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&macaddr_art_0 1>;
		nvmem-cell-names = "mac-address";
		qca,no-eeprom;
		#gpio-cells = <2>;
		gpio-controller;
	};
};
