From b8bdfc666bc5f58caf46e67b615132fccbaca3d4 Mon Sep 17 00:00:00 2001
From: Lorenzo Bianconi <lorenzo@kernel.org>
Date: Tue, 12 Nov 2024 01:08:50 +0100
Subject: [PATCH 2/6] clk: en7523: move clock_register in hw_init callback

Move en7523_register_clocks routine in hw_init callback.
Introduce en7523_clk_hw_init callback for EN7523 SoC.
This is a preliminary patch to differentiate IO mapped region between
EN7523 and EN7581 SoCs in order to access chip-scu IO region
<0x1fa20000 0x384> on EN7581 SoC as syscon device since it contains
miscellaneous registers needed by multiple devices (clock, pinctrl ..).

Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
Link: https://lore.kernel.org/r/20241112-clk-en7581-syscon-v2-3-8ada5e394ae4@kernel.org
Signed-off-by: Stephen Boyd <sboyd@kernel.org>
---
 drivers/clk/clk-en7523.c | 82 ++++++++++++++++++++++++----------------
 1 file changed, 50 insertions(+), 32 deletions(-)

--- a/drivers/clk/clk-en7523.c
+++ b/drivers/clk/clk-en7523.c
@@ -78,7 +78,8 @@ struct en_clk_soc_data {
 		const u16 *idx_map;
 		u16 idx_map_nr;
 	} reset;
-	int (*hw_init)(struct platform_device *pdev, void __iomem *np_base);
+	int (*hw_init)(struct platform_device *pdev,
+		       struct clk_hw_onecell_data *clk_data);
 };
 
 static const u32 gsw_base[] = { 400000000, 500000000 };
@@ -406,20 +407,6 @@ static void en7581_pci_disable(struct cl
 	usleep_range(1000, 2000);
 }
 
-static int en7581_clk_hw_init(struct platform_device *pdev,
-			      void __iomem *np_base)
-{
-	u32 val;
-
-	val = readl(np_base + REG_NP_SCU_SSTR);
-	val &= ~(REG_PCIE_XSI0_SEL_MASK | REG_PCIE_XSI1_SEL_MASK);
-	writel(val, np_base + REG_NP_SCU_SSTR);
-	val = readl(np_base + REG_NP_SCU_PCIC);
-	writel(val | 3, np_base + REG_NP_SCU_PCIC);
-
-	return 0;
-}
-
 static void en7523_register_clocks(struct device *dev, struct clk_hw_onecell_data *clk_data,
 				   void __iomem *base, void __iomem *np_base)
 {
@@ -449,6 +436,49 @@ static void en7523_register_clocks(struc
 	clk_data->num = EN7523_NUM_CLOCKS;
 }
 
+static int en7523_clk_hw_init(struct platform_device *pdev,
+			      struct clk_hw_onecell_data *clk_data)
+{
+	void __iomem *base, *np_base;
+
+	base = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(base))
+		return PTR_ERR(base);
+
+	np_base = devm_platform_ioremap_resource(pdev, 1);
+	if (IS_ERR(np_base))
+		return PTR_ERR(np_base);
+
+	en7523_register_clocks(&pdev->dev, clk_data, base, np_base);
+
+	return 0;
+}
+
+static int en7581_clk_hw_init(struct platform_device *pdev,
+			      struct clk_hw_onecell_data *clk_data)
+{
+	void __iomem *base, *np_base;
+	u32 val;
+
+	base = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(base))
+		return PTR_ERR(base);
+
+	np_base = devm_platform_ioremap_resource(pdev, 1);
+	if (IS_ERR(np_base))
+		return PTR_ERR(np_base);
+
+	en7523_register_clocks(&pdev->dev, clk_data, base, np_base);
+
+	val = readl(np_base + REG_NP_SCU_SSTR);
+	val &= ~(REG_PCIE_XSI0_SEL_MASK | REG_PCIE_XSI1_SEL_MASK);
+	writel(val, np_base + REG_NP_SCU_SSTR);
+	val = readl(np_base + REG_NP_SCU_PCIC);
+	writel(val | 3, np_base + REG_NP_SCU_PCIC);
+
+	return 0;
+}
+
 static int en7523_reset_update(struct reset_controller_dev *rcdev,
 			       unsigned long id, bool assert)
 {
@@ -543,31 +573,18 @@ static int en7523_clk_probe(struct platf
 	struct device_node *node = pdev->dev.of_node;
 	const struct en_clk_soc_data *soc_data;
 	struct clk_hw_onecell_data *clk_data;
-	void __iomem *base, *np_base;
 	int r;
 
-	base = devm_platform_ioremap_resource(pdev, 0);
-	if (IS_ERR(base))
-		return PTR_ERR(base);
-
-	np_base = devm_platform_ioremap_resource(pdev, 1);
-	if (IS_ERR(np_base))
-		return PTR_ERR(np_base);
-
-	soc_data = device_get_match_data(&pdev->dev);
-	if (soc_data->hw_init) {
-		r = soc_data->hw_init(pdev, np_base);
-		if (r)
-			return r;
-	}
-
 	clk_data = devm_kzalloc(&pdev->dev,
 				struct_size(clk_data, hws, EN7523_NUM_CLOCKS),
 				GFP_KERNEL);
 	if (!clk_data)
 		return -ENOMEM;
 
-	en7523_register_clocks(&pdev->dev, clk_data, base, np_base);
+	soc_data = device_get_match_data(&pdev->dev);
+	r = soc_data->hw_init(pdev, clk_data);
+	if (r)
+		return r;
 
 	r = of_clk_add_hw_provider(node, of_clk_hw_onecell_get, clk_data);
 	if (r)
@@ -590,6 +607,7 @@ static const struct en_clk_soc_data en75
 		.prepare = en7523_pci_prepare,
 		.unprepare = en7523_pci_unprepare,
 	},
+	.hw_init = en7523_clk_hw_init,
 };
 
 static const struct en_clk_soc_data en7581_data = {
