// SPDX-License-Identifier: GPL-2.0-or-later

#include "rtl8380_zyxel_gs1900.dtsi"

/ {
	compatible = "zyxel,gs1900-24e", "realtek,rtl838x-soc";
	model = "Zyxel GS1900-24E";
};

&mdio {
	EXTERNAL_PHY(0)
	EXTERNAL_PHY(1)
	EXTERNAL_PHY(2)
	EXTERNAL_PHY(3)
	EXTERNAL_PHY(4)
	EXTERNAL_PHY(5)
	EXTERNAL_PHY(6)
	EXTERNAL_PHY(7)

	EXTERNAL_PHY(16)
	EXTERNAL_PHY(17)
	EXTERNAL_PHY(18)
	EXTERNAL_PHY(19)
	EXTERNAL_PHY(20)
	EXTERNAL_PHY(21)
	EXTERNAL_PHY(22)
	EXTERNAL_PHY(23)
};

&switch0 {
	ports {
		SWITCH_PORT(1, 1, qsgmii)
		SWITCH_PORT(0, 2, qsgmii)
		SWITCH_PORT(3, 3, qsgmii)
		SWITCH_PORT(2, 4, qsgmii)
		SWITCH_PORT(5, 5, qsgmii)
		SWITCH_PORT(4, 6, qsgmii)
		SWITCH_PORT(7, 7, qsgmii)
		SWITCH_PORT(6, 8, qsgmii)

		SWITCH_PORT(9, 9, internal)
		SWITCH_PORT(8, 10, internal)
		SWITCH_PORT(11, 11, internal)
		SWITCH_PORT(10, 12, internal)
		SWITCH_PORT(13, 13, internal)
		SWITCH_PORT(12, 14, internal)
		SWITCH_PORT(15, 15, internal)
		SWITCH_PORT(14, 16, internal)

		SWITCH_PORT(17, 17, qsgmii)
		SWITCH_PORT(16, 18, qsgmii)
		SWITCH_PORT(19, 19, qsgmii)
		SWITCH_PORT(18, 20, qsgmii)
		SWITCH_PORT(21, 21, qsgmii)
		SWITCH_PORT(20, 22, qsgmii)
		SWITCH_PORT(23, 23, qsgmii)
		SWITCH_PORT(22, 24, qsgmii)
	};
};

&gpio1 {
	/delete-node/ poe_enable;
};
