From 38ea04a79ad0f8cc30bb5e9ad98d665e4ae5060c Mon Sep 17 00:00:00 2001
From: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Date: Thu, 8 Aug 2024 01:20:36 +0300
Subject: [PATCH] wifi: rtw88: usb: Update the RX stats after every frame

Update the number of received unicast data frames and bytes every time
a frame is received. This is what the PCI and SDIO drivers do.

This has an influence on the power saving, bluetooth coexistence, and
(in a future patch) the use of RX aggregation.

Tested with RTL8822CU, RTL8811CU, and RTL8723DU.

Tested-by: Sascha Hauer <s.hauer@pengutronix.de>
Signed-off-by: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Signed-off-by: Ping-Ke Shih <pkshih@realtek.com>
Link: https://patch.msgid.link/75a2ca52-8f01-45c5-926f-d3a68ae3b284@gmail.com
---
 drivers/net/wireless/realtek/rtw88/usb.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/net/wireless/realtek/rtw88/usb.c
+++ b/drivers/net/wireless/realtek/rtw88/usb.c
@@ -581,6 +581,7 @@ static void rtw_usb_rx_handler(struct wo
 		skb_reserve(skb, pkt_offset);
 
 		rtw_update_rx_freq_for_invalid(rtwdev, skb, &rx_status, &pkt_stat);
+		rtw_rx_stats(rtwdev, pkt_stat.vif, skb);
 		memcpy(skb->cb, &rx_status, sizeof(rx_status));
 		ieee80211_rx_irqsafe(rtwdev->hw, skb);
 	}
