From 8fbcaa308591b91e9037ab6a8d733873b749a70d Mon Sep 17 00:00:00 2001
From: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Date: Sat, 6 Jul 2024 01:40:58 +0300
Subject: [PATCH] wifi: rtw88: Set efuse->ext_lna_5g - fix typo

efuse->ext_lna_2g is set twice and efuse->ext_lna_5g is not set at all.
Set each one once.

Nothing uses these members right now. They will be used by the RTL8821AU
and RTL8812AU drivers.

Signed-off-by: Bitterblue Smith <rtl8821cerfe2@gmail.com>
Acked-by: Ping-Ke Shih <pkshih@realtek.com>
Signed-off-by: Ping-Ke Shih <pkshih@realtek.com>
Link: https://patch.msgid.link/8ccc9e13-0d45-417d-8f88-93a0ad294f77@gmail.com
---
 drivers/net/wireless/realtek/rtw88/main.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/wireless/realtek/rtw88/main.c
+++ b/drivers/net/wireless/realtek/rtw88/main.c
@@ -2006,7 +2006,7 @@ static int rtw_chip_efuse_info_setup(str
 	efuse->ext_pa_2g = efuse->pa_type_2g & BIT(4) ? 1 : 0;
 	efuse->ext_lna_2g = efuse->lna_type_2g & BIT(3) ? 1 : 0;
 	efuse->ext_pa_5g = efuse->pa_type_5g & BIT(0) ? 1 : 0;
-	efuse->ext_lna_2g = efuse->lna_type_5g & BIT(3) ? 1 : 0;
+	efuse->ext_lna_5g = efuse->lna_type_5g & BIT(3) ? 1 : 0;
 
 	if (!is_valid_ether_addr(efuse->addr)) {
 		eth_random_addr(efuse->addr);
