From 24b2a2bc1e1f2c64bbacec6e78b3ac94545838c1 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Fri, 6 May 2022 15:34:44 +0100
Subject: [PATCH 0369/1085] thermal: broadcom: Use dev_err_probe to suppress
 defer errors

It is quite common for the devm_thermal_zone_of_sensor_register
to need to defer, so avoid spamming the log by using
dev_err_probe instead of dev_err.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/thermal/broadcom/bcm2711_thermal.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/thermal/broadcom/bcm2711_thermal.c
+++ b/drivers/thermal/broadcom/bcm2711_thermal.c
@@ -92,7 +92,7 @@ static int bcm2711_thermal_probe(struct
 						&bcm2711_thermal_of_ops);
 	if (IS_ERR(thermal)) {
 		ret = PTR_ERR(thermal);
-		dev_err(dev, "could not register sensor: %d\n", ret);
+		dev_err_probe(dev, ret, "could not register sensor: %d\n", ret);
 		return ret;
 	}
 
