From aea9bc13e7c53b5c8fb649dddf3f776c9d2e1fb9 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Fri, 17 Feb 2023 13:36:02 +0100
Subject: [PATCH 0603/1085] dt-bindings: display: Add BCM2712 HDMI bindings

The BCM2712 HDMI controller uses a slightly different HDMI controller
than the BCM2711, and a completely different PHY.

Let's introduce a new compatible for it.

Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 .../devicetree/bindings/display/brcm,bcm2711-hdmi.yaml          | 2 ++
 1 file changed, 2 insertions(+)

--- a/Documentation/devicetree/bindings/display/brcm,bcm2711-hdmi.yaml
+++ b/Documentation/devicetree/bindings/display/brcm,bcm2711-hdmi.yaml
@@ -14,6 +14,8 @@ properties:
     enum:
       - brcm,bcm2711-hdmi0
       - brcm,bcm2711-hdmi1
+      - brcm,bcm2712-hdmi0
+      - brcm,bcm2712-hdmi1
 
   reg:
     items:
