From 16d0ee22d2c0b32cc67db73ce03263b740bba2a7 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Wed, 31 Jul 2024 15:02:47 +0100
Subject: [PATCH 1204/1215] hwmon: (adt7410) Add DT compatible strings

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 drivers/hwmon/adt7410.c | 8 ++++++++
 1 file changed, 8 insertions(+)

--- a/drivers/hwmon/adt7410.c
+++ b/drivers/hwmon/adt7410.c
@@ -94,10 +94,18 @@ static const struct i2c_device_id adt741
 };
 MODULE_DEVICE_TABLE(i2c, adt7410_ids);
 
+static const struct of_device_id adt7410_of_ids[] = {
+	{ .compatible = "adi,adt7410" },
+	{ .compatible = "adi,adt7420" },
+	{}
+};
+MODULE_DEVICE_TABLE(of, adt7410_of_ids);
+
 static struct i2c_driver adt7410_driver = {
 	.class		= I2C_CLASS_HWMON,
 	.driver = {
 		.name	= "adt7410",
+		.of_match_table = adt7410_of_ids,
 		.pm	= pm_sleep_ptr(&adt7x10_dev_pm_ops),
 	},
 	.probe		= adt7410_i2c_probe,
